Montana Rockworks Distributed by ZeroDocs.com

**SECTION 04 44 00 – COLLECTED STONE**

1. **GENERAL**
	1. SUBMITTALS
		1. Action Submittals:
			1. Samples: [Selection samples.] [Verification samples.]
	2. QUALITY ASSURANCE
		1. Mockup: [One stone.] [[\_\_\_\_] stones.] Approved mockup [may] [may not] remain as part of the Work.
2. **PRODUCTS**
	1. MANUFACTURERS
		1. Contract Documents are based on products by Montana Rockworks. [www.montanarockworks.com](http://www.montanarockworks.com).

* + 1. Substitutions: [Refer to Division 01.] [Not permitted.]
	1. MATERIALS
		1. Collected Stone:
			1. Color: [\_\_\_\_].
			2. Nominal sizes: [\_\_] to [\_\_] [feet.] [inches.]
	2. ACCESSORIES
		1. Mortar: ASTM C270, Type S, [gray.] [[\_\_\_\_] color.]
1. **EXECUTION**
	1. PREPARATION
		1. Compact soil to receive stones to minimum 95 percent of ASTM D698 standard proctor density at or near optimum moisture content.
	2. INSTALLATION
		1. Orient stones for best appearance.
		2. Obtain [Landscape Architect's] [\_\_\_\_] approval of location and appearance.
		3. Place stones on compacted soil with full bearing, free from rocking.

\*\*\*\* OR \*\*\*\*

* + 1. Set stones on full mortar bed.

END OF SECTION