The following specification text has been prepared by D&D Technologies to assist design professionals in the preparation of a specification section covering SureClose ConcealFit Closer + Hinge Kit, SureClose ConcealFit Hinge, and SureClose ConcealFit Weld-On Gate Mounting Boxes.

Utilize these paragraphs to insert text into Specification Section 08 71 00 – Door Hardware, 32 31 00 – Fences and Gates, or other section governing this work.

Optional text requiring a selection by the user is enclosed within brackets and as red text, e.g.: Color: [Red.] [Black.]"

For assistance on the use of the products in this section, call 800-716-0888 or visit the D&D Technologies website at [www.us.ddtech.com](http://www.us.ddtech.com).

PART 1 – GENERAL

SUBMITTALS

A. Action Submittals:

1. Product Data: Manufacturer’s descriptive data and product attributes.

2. Samples: One sample of each component, if requested.

WARRANTY

 A. Manufacturer’s warranty to original purchaser against defects in materials and workmanship.

PART 2 – PRODUCTS

COMPONENTS

1. Combination Closer/Hinge:
	* + 1. Source: SureClose ConcealFit Closer + Hinge Kit by D&D Technologies. [www.us.ddtech.com](http://www.us.ddtech.com)
			2. Description: Maintenance-free door closer and hinge combination with soft, controlled closing and removable cover concealing adjustment screws and valves.
			3. Mounting: Mortised into door or door frame.

1. Concealed Hinge:
2. Source: SureClose ConcealFit Hinge by D&D Technologies. [www.us.ddtech.com](http://www.us.ddtech.com).
3. Description: Maintenance-free door hinge, non-self-closing, with removable cover concealing adjustment screws.
4. Mounting: Mortised into door or door frame.
5. Gate Mounting Boxes:
6. Source: ConcealFit Weld-On Gate Mounting Boxes by D&D Technologies. [www.us.ddtech.com](http://www.us.ddtech.com)
7. Description: [Steel with zinc plated finish,] [Aluminum, mill finish,] formed with recess to receive ConcealFit hinge or closer.
8. Mounting: Welded to gate frame or fence post.

PART 3 – EXECUTION

INSTALLATION

 A. Install in accordance with manufacturer’s instructions.