Panoramic Doors Distributed by ZeroDocs.com

SECTION 08 35 14 –VINYL FOLDING DOORS

GENERAL

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes for entrances.

Samples: [Selection samples.] [Verification samples.]

Informational Submittals:

Certificate of Compliance: Certification that installed products meet specified design and performance requirements.

SYSTEM DESCRIPTION

Vinyl Folding Doors:

AAMA/WDMA/CSA - 101/I.S.2/A440 with Canadian Supplement A440S1, Performance Grade DP30; Canadian Air Infiltration/Exfiltration Level A2.

Air leakage: Maximum 0.17 CFM per square foot, tested to ASTM E283 at 1.57 PSF.

Water penetration: No uncontrolled water leakage, tested to ASTM E547 at 7.52 PSF.

Forced entrance resistance: Conform to AAMA 1304.

System Operation:

Master swing door on every door system.

Individually moving panels.

Hingeless operation.

Bottom track supported.

Interlocking panels.

[Inswing] [Outswing] panels.

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

Mockup: [One full sized door unit.] [\_\_\_\_.] Approved mockup [may] [may not] remain as part of the Work.

WARRANTIES

Manufacturer’s warranty providing following coverages:

Defects in materials or workmanship: 10 years.

Hardware: 5 years.

[PVC] [Laminated] finishes: [1 year.] [10 years.]

Insulated glass units: 10 years.

PRODUCTS

MANUFACTURERS

Contract Documents are based on Absolute Series vinyl folding doors by Panoramic Doors, [www.panoramicdoors.com](http://www.panoramicdoors.com).

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

[Vinyl:] [Laminated Vinyl:] Manufacturer’s standard; heat and ultraviolet resistant.

Glass:

Description: ASTM E2190, 1 inch thick sealed insulating.

Glass type: ASTM C1048, Kind FT fully tempered.

Interior lite: Clear.

Exterior lite: [Clear.] [[\_\_\_\_] tinted.]

Low-e-coating: Located on [No. 2] [No. 3] surface.

Hardware:

Door handles: [Lakeview Black.] [Lakeview Silver.] [Estate Black.] [Estate Silver.] [Cityscape White.]

Locking: Multipoint locking mechanism.

Bottom track: [Upstand] [Flush] type.

Retractable Screens: Extruded aluminum frame with pleated screen, manually operated.

FABRICATION

Size and Configuration: [\_\_\_\_.] [Refer to Drawings.]

Laminated Vinyl Doors: Provide lamination on [interior side] [exterior side] [both sides of door.]

FINISHES

Vinyl: [White.] [Beige.]

\*\*\*\* OR \*\*\*\*

Laminated Vinyl: [Black.] [Bronze.] [Silver.] [Anthracite Gray.]

EXECUTION

INSTALLATION

Install in accordance with manufacturer's instructions and approved Shop Drawings.

Installation Tolerances:

Maximum variation from plumb or level: [1/16] [\_\_] inch in 3 feet or [1/8] [\_\_] inch in any 10 feet, whichever is less.

Maximum misalignment of members abutting end to end: [1/32] [\_\_] inch.

Sealant space between system and adjacent construction: [3/8] [\_\_] inch plus or minus [1/8] [\_\_] inch.

END OF SECTION