Scepter Developed by ZeroDocs.com

SECTION 01 56 26 – TEMPORARY FENCING

 GENERAL

 ADMINISTRATIVE REQUIREMENTS

 Pre-Installation Conference:

 Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] and fence installer.

 Review: Project conditions, proposed fencing locations, and installation schedule.

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes.

 Samples: Verification samples.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by Scepter, [www.scepterposts.com](http://www.scepterposts.com).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 COMPONENTS

 Fence Posts:

 Product: Scepter Post, Multi-Fence Heavy Duty.

 Length: 60 inches.

\*\*\*\* OR \*\*\*\*

 Fence Posts:

 Product: Scepter Post, Standard Heavy Duty.

 Length: 60 inches.

\*\*\*\* OR \*\*\*\*

 Fence Posts:

 Product: Scepter Post, Multi-Fence Lite.

 Length: 60 inches.

\*\*\*\* OR \*\*\*\*

 Fence Posts:

 Product: Scepter Post, Standard Lite.

 Length: 60 inches.

\*\*\*\* OR \*\*\*\*

 Fence Posts:

 Product: Scepter Post, Silt Pole HD.

 Length: 39.4 inches.

 Fence Mesh:

 Product: Barrier Fence.

 Height: 48 inches.

 Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

 Fence Mesh:

 Product: Barricade Fence.

 Height: 48 inches.

 Opening size: 1.5 x 2.5 inches.

 Thickness: 0.0125 inch.

 \*\*\*\* OR \*\*\*\*

 Fence Mesh:

 Product: Snow Control Fence.

 Height: 48 inches.

\*\*\*\* OR \*\*\*\*

 Fence Mesh:

 Product: Snow Fence.

 Height: 48 inches.

 Opening size: 1.25 x 2 inches.

\*\*\*\* OR \*\*\*\*

 Fence Mesh:

 Product: Yard Fence.

 Height:48 inches.

 Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

 Fence Fabric:

 Product: Silt Fence.

 Height: 36 inches.

 Sieve size: No. 30 (0.023 inch).

 Caution Tape:

 Product: Caution Tape.

 Height: \_\_\_\_ inches.

 Color: [Red.] [Yellow.]

 Lettering: [CAUTION.] [DANGER.] [DO NOT ENTER.]

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions.

 Maximum fence post spacing: [\_\_] feet on center.

END OF SECTION