Alta Products Developed by ZeroDocs.com

SECTION 07 23 16 – MANUFACTURED ROOF PIPE CHASES

 GENERAL

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes.

 QUALITY ASSURANCE

 Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

 WARRANTIES

 Pipe Chases: Manufacturer’s 20 year warranty against defects in materials and workmanship.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by Alta Products, [www.altaproductsllc.com](http://www.altaproductsllc.com).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MANUFACTURED UNITS

 Manufactured Roof Pipe Chases:

 Product: Sigrist Pipe Chase Housing.

 Construction:

* + - * 1. Housing and curb: [0.080] [0.125] inch thick aluminum sheet with UV-protected powder coated finish.
				2. Fasteners: Stainless steel.
				3. Full thermal break in housing, curb, and lid interior.
				4. Gaskets between lid-to-housing and housing-to-curb connection points.

 Size: [Small, 16.5 x 10 inches x 12.5 inches high.] [Medium, 20.5 x 14.5 inches x 13.5 inches high.] [Medium Double Long, 38 x 14.5 inches x 13.5 inches high.] [Large, 34 x 34 inches x 24 inches high.] [Data Center, 18 x 60 inches x 24 inches high.] [TYM, 48 x 48 x 24 inches high.]

 Curb height: [14] [18] [24] inches.

 Pipe Seals:

 Product: Sigrist Exit Seal.

 Construction: Injection molded, UV-inhibited resin with EPDM gaskets.

 Pathway size: [To suit pipe or conduit size.] [[\_\_] inches.]

 Length: [Standard.] [X-Long.]

 ACCESSORIES

 Fasteners: [Corrosion-resistant coated steel.] [Series 300 stainless steel.]

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions.

END OF SECTION