Alta Products Developed by ZeroDocs.com

SECTION 07 23 16 – MANUFACTURED ROOF PIPE CHASES

GENERAL

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes.

QUALITY ASSURANCE

Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

WARRANTIES

Pipe Chases: Manufacturer’s 20 year warranty against defects in materials and workmanship.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by Alta Products, [www.altaproductsllc.com](http://www.altaproductsllc.com).

Substitutions: [Refer to Division 01.] [Not permitted.]

MANUFACTURED UNITS

Manufactured Roof Pipe Chases:

Product: Sigrist Pipe Chase Housing.

Construction:

* + - * 1. Housing and curb: [0.080] [0.125] inch thick aluminum sheet with UV-protected powder coated finish.
        2. Fasteners: Stainless steel.
        3. Full thermal break in housing, curb, and lid interior.
        4. Gaskets between lid-to-housing and housing-to-curb connection points.

Size: [Small, 16.5 x 10 inches x 12.5 inches high.] [Medium, 20.5 x 14.5 inches x 13.5 inches high.] [Medium Double Long, 38 x 14.5 inches x 13.5 inches high.] [Large, 34 x 34 inches x 24 inches high.] [Data Center, 18 x 60 inches x 24 inches high.]

Curb height: [14] [18] [24] inches.

Pipe Seals:

Product: Sigrist Exit Seal.

Construction: Injection molded, UV-inhibited resin with EPDM gaskets.

Pathway size: [To suit pipe or conduit size.] [[\_\_] inches.]

Length: [Standard.] [X-Long.]

ACCESSORIES

Fasteners: [Corrosion-resistant coated steel.] [Series 300 stainless steel.]

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions.

END OF SECTION