M-D PRO Distributed by ZeroDocs.com

SECTION 09 28 23 – TILE BACKING BOARDS

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes.

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by M-D PRO, [www.mdpro.com/prova](http://www.mdpro.com/prova).

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Tile Backing Boards:

Product: Prova Board Plus.

Description: Waterproof extruded polystyrene core faced both sides with woven mesh and cementitious coating.

Meet IAPMO PS 106.

Thickness: [1/8” (3.2 mm)] [1/4” (6.4 mm)] [1/2” (12.7 mm)] [2” (5 cm)]

ACCESSORIES

Fasteners: ASTM C1513 screws, hot-dip galvanized or fluoropolymer coated steel.

EXECUTION

INSTALLATION

Install in accordance with manufacturer's instructions.

Fasten panels to framing at maximum [12” (30 cm)] [16” (41 cm)] [\_\_] on center.

END OF SECTION