M-D PRO Distributed by ZeroDocs.com

SECTION 09 28 23 – TILE BACKING BOARDS

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes.

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by M-D PRO, [www.mdpro.com/prova](http://www.mdpro.com/prova).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Tile Backing Boards:

 Product: Prova Board Plus.

 Description: Waterproof extruded polystyrene core faced both sides with woven mesh and cementitious coating.

 Meet IAPMO PS 106.

 Thickness: [1/8” (3.2 mm)] [1/4” (6.4 mm)] [1/2” (12.7 mm)] [2” (5 cm)]

 ACCESSORIES

 Fasteners: ASTM C1513 screws, hot-dip galvanized or fluoropolymer coated steel.

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer's instructions.

 Fasten panels to framing at maximum [12” (30 cm)] [16” (41 cm)] [\_\_] on center.

END OF SECTION