M-D PRO Distributed by ZeroDocs.com

SECTION 09 30 43 – TILING ACCESSORIES

1. GENERAL
	1. SUBMITTALS
		1. Action Submittals:
			1. Product Data: Manufacturer’s descriptive data and product attributes.
	2. QUALITY ASSURANCE
		1. Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.
2. PRODUCTS
	1. MANUFACTURERS
		1. Contract Documents are based on products by M-D PRO, [www.mdpro.com/prova](https://www.mdpro.com/prova)
		2. Substitutions: [Refer to Division 01.] [Not permitted.]
	2. MATERIALS
		1. Tile Underlayment:
			1. Product: Prova-Flex.
			2. Description: Lightweight uncoupling membrane.
			3. Comply with ANSI A118.12.
			4. Rating: Extra Heavy Performance Rating, tested to ASTM C627.
			5. Thickness: 0.16” (4 mm).

\*\*\*\* OR \*\*\*\*

* + 1. Tile Underlayment:
			1. Product: Prova Flex-Heat.
			2. Description: Lightweight uncoupling membrane with heating cable capabilities.
			3. Comply with ANSI A118.12.
			4. Rating: Extra Heavy Performance Rating, tested to ASTM C627.
			5. Thickness: 0.26” (6.5 mm).

\*\*\*\* OR \*\*\*\*

* + 1. Tile Underlayment:
			1. Product: Protegga Plus.
			2. Description: Lightweight uncoupling membrane.
			3. Comply with ANSI A118.12.
			4. Rating: Extra Heavy Performance Rating, tested to ASTM C627.
			5. Thickness: 0.16” (4 mm).
		2. Shower Pan:
			1. Product: Prova Pan.
			2. Description: Prefabricated sloped shower pan.
			3. Density: 2.75 lb./ft.3 (44.05 kg/m3).
			4. Size and drain location: [48” x 48” (122 cm x 122 cm), center drain.] [32” x 60” (81 cm x 152 cm), offset drain.] [32” x 60” (81 cm x 152 cm), center drain.]
			5. Accessories: Prova Pan Extension, as required to suit project conditions.
		3. Shower Pan:
			1. Product: Prova Pan-Multi.
			2. Description: Prefabricated sloped shower pan.
			3. Density: 3.5 lb./ft.3 (56.06 kg/m3).
			4. Size: 60” x 60” x 7/8” thick (152 cm x 152 cm x 2.2 cm thick).
			5. Drain location: Center.
			6. Extensions: Prova Pan-Multi Extension, as required to suit project conditions.

\*\*\*\* OR \*\*\*\*

* + 1. Shower Pan:
			1. Product: Prova Linear Pan.
			2. Description: Prefabricated linear sloped shower pan.
			3. Density: 2.75 lb./ft.3 (44.05 kg/m3).
			4. Size: 22.5” x 24” x 1-5/8” thick (57 cm x 61 cm x 4.1 cm thick).
			5. Accessories: Provide as required to suit project conditions.
				1. Prova Linear Pan Extension.
				2. Side supports.
				3. Filler strips.
		2. Shower Waterproofing:
			1. Product: Prova-Mat.
			2. Description: Low-perm waterproofing membrane.
			3. Comply with ANSI A118.10.
			4. Water vapor transmission: Maximum 0.115 perms, tested to ASTM E96/E96M.
			5. Thickness: 0.43 mm.
			6. Accessories:
				1. Joint sealing strip: Prova Joint.
				2. Prefabricated corners: ProvaCorner.
				3. Pipe seal: Prova Pipe Seal.
		3. Shower Drains:
			1. Product: Prova Drain.
			2. Description: Coated [ABS] [PVC] drain body with [stainless steel] [chrome] [brass] [bronze] graphite] [black] drain cover.
			3. Meet ASME A112.18.2-2020/CSA B125.2-20.
		4. Shower Drains:
			1. Product: Prova Drain Plus.
			2. Description: Coated [ABS] [PVC] drain body with [stainless steel] [chrome] [brass] [bronze] graphite] [black] drain cover.
			3. Meet ASME A112.18.2-2020/CSA B125.2-20.
			4. Adapter ring for connection to existing components of 3-piece/clamping ring drains.
		5. Linear Drains:
			1. Product: Prova Linear Drain.
			2. Description: Coated drain body with waterproofing membrane adhered to drain flange.
			3. Meet ASME A112.18.2-2020/CSA B125.2-20.
			4. Width: [24” (61 cm)] [36” (91 cm)] [42” (107 cm)].
			5. Drain grate: Prova Linear Grate.
		6. Prefabricated Niches:
			1. Product: Prova Niche.
			2. Description: Prefabricated tile backing board.
			3. Meet IAPMO PS 106.
			4. Inside dimensions: [16” x 16” (40.6 cm x 40.6 cm)] [24” x 16” (61 cm x 40.6 cm)] [33” x 16” (83.8 cm x 40.6 cm)].
			5. Shelves: [None.] [3/8” (9.5 mm) thick clear laminated glass shelves, [one] [two] per niche.]
		7. Prefabricated Shower Curbs:
			1. Product: Prova Curb.
			2. Description: Prefabricated expanded polystyrene low-profile shower curb.
			3. Density: 3.0 PCF.
			4. Size: 4-1/2” (11 cm) x 4” (10 cm) x [48” (122 cm)] [60” (152 cm)] long.
		8. Tile Edgings:
			1. Product: Prova Tile Edge.
			2. Material: Aluminum.
			3. Color and finish: [Mill finish.] [Anodized, [brushed] [bright] finish, [\_\_\_\_] color [to be selected from manufacturer’s full color range.] [Powder coated, [\_\_\_\_] color [to be selected from manufacturer’s full color range.]
			4. Profiles:
				1. Flat Tile Edge.
				2. Round Tile Edge.
				3. Round Outside Corner.
				4. Round Inside Corner.
				5. Square Tile Edge.
				6. Square Corner.
				7. Ceramic Cove.
				8. Ceramic Cove Corner.
				9. J-Molding.
				10. Ceramic Adapter.
				11. Ceramic Reducer.
				12. Ceramic Tile Stair Nosing.
				13. Decorative Tile Stair Nosing.
				14. Dual-Purpose Decorative Edging.
				15. Counter Top/Stair Nosing.
				16. Counter Top Corner.
				17. T-Molding.
				18. T-Molding Reducer.
				19. Anti-Skid Stair nosing with vinyl insert.
				20. Ceramic Edge Protection Ramp.
				21. Heavy-Duty Expansion Joint with vinyl insert.

\*\*\*\* OR \*\*\*

* + 1. Tile Edgings:
			1. Material: Stainless steel.
			2. Profiles:
				1. Flat Tile Edge.
				2. Round Tile Edge.
				3. Round corner.
				4. Square Tile Edge.
				5. Square Corner.

\*\*\*\* OR \*\*\*\*

* + 1. Tile Edgings:
			1. Material: PVC.
			2. Profiles:
				1. Vinyl Tile Edge.
				2. Vinyl J-Cap.
				3. Heavy Duty Vinyl Edge – Flat.
				4. Heavy Duty Vinyl Edge – Round.
				5. Round Corner.
				6. Expansion Joint.
1. EXECUTION
	1. INSTALLATION
		1. Install in accordance with manufacturer's instructions.

END OF SECTION