M-D PRO Distributed by ZeroDocs.com

SECTION 09 65 13 - RESILIENT BASE

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes for base.

 Samples: [Selection samples.] [Verification samples.]

 Closeout Submittals:

 Extra materials: [One unopened carton] [[\_\_] unopened cartons] [[2] [\_\_] percent] [[\_\_] linear feet] of each base.

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by M-D PRO. [www.mdpro.com/flooring](http://www.mdpro.com/flooring)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Resilient Base:

 Meet ASTM F1861.

 Composition: [Vinyl.] [Rubber.]

 Profile: [Straight.] [Coved.]

 Height: [2-1/2” (63.5 mm)] [4” (101.6 mm)] [6” (152.4 mm)].

 Thickness: [0.080” (2.03 mm)] [0.125” (3.2 mm)].

 Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

 Premolded corners: Size and color to match base.

\*\*\*\* OR \*\*\*\*

 Resilient Base:

 Meet ASTM F1861.

 Composition: Heavy gauge designer vinyl.

 Profile: Estate.

 Height: 4-1/2” (11.4 cm).

 Thickness: 3/8” (9.5 mm).

 Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

 Finish: Satin.

\*\*\*\* OR \*\*\*\*

 Resilient Base:

 Meet ASTM F1861.

 Composition: Heavy gauge designer vinyl.

 Profile: Contemporary.

 Height: [4-1/4” (10.8 cm)] [4-1/2” (11.4 cm)].

 Thickness: [5/16” (7.9 mm)] [3/8” (9.5 mm)].

 Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

 Finish: Satin.

\*\*\*\* OR \*\*\*\*

 Resilient Base:

 Meet ASTM F1861.

 Composition: Heavy gauge designer vinyl.

 Profile: Pinnacle.

 Height: 4-1/2” (11.4 cm).

 Thickness: 1/4" (6.4 mm).

 Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

 Finish: Satin.

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions.

END OF SECTION