M-D PRO Distributed by ZeroDocs.com

SECTION 09 65 13 - RESILIENT BASE

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes for base.

Samples: [Selection samples.] [Verification samples.]

Closeout Submittals:

Extra materials: [One unopened carton] [[\_\_] unopened cartons] [[2] [\_\_] percent] [[\_\_] linear feet] of each base.

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by M-D PRO. [www.mdpro.com/flooring](http://www.mdpro.com/flooring)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Resilient Base:

Meet ASTM F1861.

Composition: [Vinyl.] [Rubber.]

Profile: [Straight.] [Coved.]

Height: [2-1/2” (63.5 mm)] [4” (101.6 mm)] [6” (152.4 mm)].

Thickness: [0.080” (2.03 mm)] [0.125” (3.2 mm)].

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

Premolded corners: Size and color to match base.

\*\*\*\* OR \*\*\*\*

Resilient Base:

Meet ASTM F1861.

Composition: Heavy gauge designer vinyl.

Profile: Estate.

Height: 4-1/2” (11.4 cm).

Thickness: 3/8” (9.5 mm).

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

Finish: Satin.

\*\*\*\* OR \*\*\*\*

Resilient Base:

Meet ASTM F1861.

Composition: Heavy gauge designer vinyl.

Profile: Contemporary.

Height: [4-1/4” (10.8 cm)] [4-1/2” (11.4 cm)].

Thickness: [5/16” (7.9 mm)] [3/8” (9.5 mm)].

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

Finish: Satin.

\*\*\*\* OR \*\*\*\*

Resilient Base:

Meet ASTM F1861.

Composition: Heavy gauge designer vinyl.

Profile: Pinnacle.

Height: 4-1/2” (11.4 cm).

Thickness: 1/4" (6.4 mm).

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

Finish: Satin.

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions.

END OF SECTION