Barron Designs Developed by ZeroDocs.com

SECTION 06 61 16 – SIMULATED [STONE] [BRICK] COLUMN COVERS

GENERAL

ADMINISTRATIVE REQUIREMENTS

Pre-Installation Conference:

Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] installer, and related trades.

Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes.

Samples: Verification samples.

Informational Submittals:

Certificate of Compliance: Certification that installed products meet specified fire hazard classification.

QUALITY ASSURANCE

Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

Fire Hazard Classification: Maximum flame spread/smoke developed rating of 25/450, tested to ASTM E84.

Mockup: [One] [\_\_\_\_] full size column cover. Approved mockup [may] [may not] remain as part of the Work.

WARRANTY

Manufacturer’s standard 15-year warranty for manufacturing defects.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by Barron Designs, [www.barrondesigns.com](http://www.barrondesigns.com).

Substitutions: [Refer to Division 01.] [Not permitted.]

COMPONENTS

Simulated Stone Column Covers:

Material: Polyurethane.

Style: [Colorado Dry Stack Stone, Medium.] [Colorado Dry Stack Split, Narrow.] [Colorado Dry Stack, Medium/Tall.]

Style: [Windsor Split, Narrow.] [Windsor, Narrow, One Piece.] [Windsor, Medium.]

Style: [Wellington, Wide.] [Wellington, Medium.]

Style: [Tumbled Stone, Narrow, One Piece.]

Style: [Ashford Ledgestone, Wide, One Piece.]

Style: [Carlton Hampton Cobblestone, Narrow, One Piece.] [Carlton Hampton Cobblestone, Narrow.] [Carlton Hampton Cobblestone, Medium, One Piece.] [Carlton Lehigh Cobblestone, Wide, One Piece.] [Carlton Lehigh Cobblestone, Medium, One Piece.] [Carlton Castle Rock, Medium, One Piece.] [Carlton Castle Rock, Wide, One Piece.]

Impact resistance: Minimum 60 inch-pounds, tested to ASTM E2486.

Mold resistance: 10, tested to ASTM D3273.

Color: [\_\_\_\_.]

Accessories:

* + - * 1. Caps: [Colorado Dry Stack 6 Inch Split Post Cap, Medium.] [Colorado Dry Stack 6 Inch Split Post Cap, Narrow.] [Colorado Dry Stack 4 Inch Split Post Cap, Narrow.] [Colorado Dry Stack Solid, Medium.] [Colorado Dry Stack Solid, Narrow.]
        2. Caps: Tumbled Stone.
        3. Caps: [Windsor Column Cap, Narrow.] [Windsor Column Cap, Medium.]
        4. Caps: [Carlton Peaked, Medium.] [Carlton Live Edge.] [Carlton Flat, Medium.] [Carlton Crown, Wide.] [Carlton Crown, Narrow.] [Carlton Live Edge, Narrow.] [Carlton Pyramid, Narrow.] [Carlton Pyramid, Wide.]
        5. Caps: [Ashford Ledgestone, Flat, Wide.] [Ashford Ledgestone, Wide.] [Ashford Pyramid, Wide.]
        6. Caps: [Wellington, Wide.] [Wellington, Medium.]
        7. Stack sections: Ashford Ledgestone, Wide.
        8. Risers: Tumbled Stone.
        9. Pedestals: [Carlton Base, Narrow.] [Carlton Base, Wide.] [Carlton Base, Wide and Tall.]

Simulated Brick Column Covers:

Material: Polyurethane.

Style: [Carlton Traditional Brick, Narrow, One Piece.] [Carlton Traditional Brick, Medium, One Piece.] [Carlton Traditional Brick, Wide, One Piece.]

Impact resistance: Minimum 60 inch-pounds, tested to ASTM E2486.

Mold resistance: 10, tested to ASTM D3273.

Color: [\_\_\_\_.]

ACCESSORIES

Adhesive and Fasteners: Types recommended by column cover manufacturer.

Joint Sealer: Textured, color matched to column cover, type recommended by column cover manufacturer.

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions.

END OF SECTION