ASTA America Developed by ZeroDocs.com

SECTION 08 33 23.07 – COILING SHEET DOORS

 GENERAL

 ADMINISTRATIVE REQUIREMENTS

 Pre-Installation Conference:

 Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] installer, and related trades.

 Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes.

 Samples: [Selection samples.] [Verification samples.]

 Closeout Submittals:

 Operation and Maintenance Data.

 QUALITY ASSURANCE

 Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

 SYSTEM DESCRIPTION

 Design Requirements: Positive and negative design wind loads of [52.50 PSF.] [\_\_\_\_.]

 Operation: Chain hoist.

 WARRANTY

 Manufacturer’s 2 year warranty against defects in materials and workmanship.

 Manufacturer’s 40 year warranty for coating film integrity and 35 year warranty against chalking and fading of coating.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on Series 203 by ASTA America, [www.astaamerica.com](http://www.astaamerica.com).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Galvanized Steel: ASTM A653/A653M, Structural Quality, G60 coating class.

 COMPONENTS

 Curtain:

 Material: 26 gage galvanized steel.

 Profile: Continuously corrugated.

 Side stripping: Continuous rubber attached to curtain edges.

 Bottom bar: 2 x 2 inch x 3/16 inch thick galvanized steel angle, with rubber bottom seal.

 Windlocks: 10 gage steel, riveted to curtain edge.

 Drum Assembly:

 26 gage galvanized steel sheet rolled around and attached to stamped 18 gage galvanized steel drums.

 Deflection: Maximum 0.03 inch per foot of door width.

 Springs: Helical torsion type, oil tempered wire, 12,500 cycle life, mounted on 1-5/16 inch, 14 gage galvanized steel tubing.

 Guides: 12 gage galvanized steel channels [with brush seal].

 Top Draft stop: Rubber seal attached to top of curtain.

 Support Brackets: Steel.

 Lock: [Galvanized steel slide bolt attached to bottom angle, with padlock provisions.] [Chain lock.]

 Operator: [Manaras Model OMH-6112.] [Manaras Model OPH-6112.] LiftMaster Model LJ8950W.] [LiftMaster Model MH.] [LiftMaster Model H.]

 FINISHES

 Galvanized Steel: Baked epoxy primer and polyester topcoat, [\_\_\_\_] color [to be selected from manufacturer’s full color range].

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions and approved Shop Drawings.

END OF SECTION