Barron Designs Developed by ZeroDocs.com

SECTION 06 10 66 –WOOD STRUCTURAL MEMBERS

 GENERAL

 ADMINISTRATIVE REQUIREMENTS

 Pre-Installation Conference:

 Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] installer, and related trades.

 Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes.

 Samples: Verification samples.

 Closeout Submittals:

 Maintenance Data.

 QUALITY ASSURANCE

 Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

 Mockup: [One] [\_\_\_\_] full size [beam] [truss]. Approved mockup [may] [may not] remain as part of the Work.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by Barron Designs, 800-651-4223, [www.barrondesigns.com](http://www.barrondesigns.com).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 COMPONENTS

 Wood Beams:

 Size: [\_\_] inches wide x [\_\_] inches high x [[\_\_] feet long.] [length indicated.]

 Number of sides: [3.] [4.]

 End caps: [None.] [One.] [Two.]

 Color: [\_\_\_\_.]

 Style: [Barn Board] [Heavy Hand Hewn] [Traditional Hand Hewn] [Wire Brushed]

 Accessories:

* + - * 1. Beam straps: [Classic Clavos Straps.] [Custom Flexible Beam Straps.]
				2. Beam plates: [2] [4] [6] inches wide.
				3. Beam hangers: Straight Beam Hangers.
				4. Faux iron bolts.
				5. Faux iron nuts.
				6. Custom flexible beam straps, plain.
				7. Custom flexible beam straps with nuts and bolts.
				8. Custom flexible beam straps with clavos.
				9. Faux iron clavos.

 Wood Trusses:

 Design: [Arched Cord King Post with Arched Diagonals.] [Arched Cord King Post with Straight Diagonals.] [Arched Raised Cord King Post with Straight Diagonals.] [Arched Raised Cord King Post with Tail.] [Hammer Beam with Rafter Tails.] [King Post with Arched Diagonals.] [King Post with Straight Diagonals.] [Modified Two Tier King.] [Raised Cord King Post with Straight Diagonals.] [Scissor.] [Split Cord King Post with Struts and Tails.] [Raised Cord King Post with Tail.]

 Color: [\_\_\_\_.]

 ACCESSORIES

 Fasteners: Types recommended by simulated wood structural member manufacturer.

 Joint Sealer: Textured, color matched to wood components, type recommended by wood structural member manufacturer.

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions.

END OF SECTION