M-D PRO Distributed by ZeroDocs.com

SECTION 09 65 15 - RESILIENT STAIR TREADS AND NOSINGS

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes.

Samples: [Selection samples.] [Verification samples.]

Closeout Submittals:

Maintenance Data.

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by M-D PRO. [www.mdpro.com/flooring](http://www.mdpro.com/flooring)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Stair Treads:

Composition: High resin content vinyl.

Profile: [ST5010.] [ST5010SA - single abrasive strip.] [ST5010DA – double abrasive strip.]

Top surface: Safety grip rib pattern.

Thickness: Tapered from 0.25” (6.4 mm) to 0.055” (1.4 mm).

Depth: 12-1/4” (31.1 cm).

Nosing height: 2” (5.1 cm).

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

Stair Treads:

Composition: High resin content vinyl.

Profile: [ST5030.] [ST5030SA - single abrasive strip.]

Top surface: Safety grip rib pattern.

Thickness: Tapered from 0.25” (6.4 mm) to 0.045” (1.1 mm).

Depth: 12-1/4” (31.1 cm).

Nosing height: 2” (5.1 cm).

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

Stair Risers:

Composition: High resin content vinyl.

Thickness: 7/64” (2.8 cm).

Depth: 7-1/2” (19.1 cm).

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.] [To match stair treads.]

Stair Nosings:

Composition: High resin content vinyl.

Profile: Drop overlap, [NS4010; 1-5/8” (4.1 cm) high x 1-1/2” (3.8 cm) deep.] [NS4020; 1-7/8” (4.8 cm) high x 1-7/8” (4.8 cm) deep.] [NS4023; 2” (5.1 cm) high x 1-7/8” (4.8 cm) deep.]

\*\*\*\* OR \*\*\*\*

Profile: Drop butt, NS4120; 2” (5.1 cm) high x 1-7/8” (4.8 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Butt, NS4121; 2-1/8” (5.4 cm) high x 2-3/4” (7 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Over-the-top, NS4122; 2” (5.1 cm) high x 3” (7.6 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Bullnose, NS4024; 1-3/16” (3 cm) high x 1-5/8” (4.1 cm) deep with 5/8” (1.6 cm) return.

\*\*\*\* OR \*\*\*\*

Profile: Square nose, NS4030; 1-1/8” (2.9 cm) high x 1-3/8” (3.5 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Overlap nosing, NS4700; 2-3/8” (6 cm) high x 2-3/8” (6 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Insert, NT4220; 2-1/8” (5.4 cm) high x 2” (5.1 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Double insert, NT4230; 1” (2.5 cm) high x 2” (5.1 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Single butt, NT4310; 1-3/4” (4.5 cm) high x 2” (5.1 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Double butt, NT4320; 1-1/2” (3.8 cm) high x 2” (5.1 cm) deep.

\*\*\*\* OR \*\*\*\*

Profile: Butt, NT4330; 2” (5.1 cm) high x 2” (5.1 cm) deep.

Color: [\_\_\_\_.] [To be selected from manufacturer's full color range.]

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions.

Fit resilient accessories tight to [treads] [risers] [and] [stringers].

END OF SECTION