SECTION 06 46 00 - WOOD TRIM

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes for trim.

 Samples: [Selection samples.] [Verification samples.]

 ADMINISTRATIVE REQUIREMENTS

 Pre-Installation Conference:

 Attendance: [Design Professional,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder,] installer, and related trades.

 Review: Critical dimensions, delivery and storage, staging and sequencing, and protection of completed work.

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

 Mockups: [[8] [\_\_] feet long.] [\_\_\_\_.] Approved mockups [may] [may not] remain as part of the Work.

 WARRANTIES

 Manufacturer’s 15 year warranty against peeling, checking, and chalking.

\*\*\*\* OR \*\*\*\*

 Manufacturer’s 40 year warranty against rot, decay, and damage by insects or termites.

 PRODUCTS

 MANUFACTURERS

 Wood Trim: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 [Interior] [Exterior] Trim:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Pine.

 Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

 Profile: Tongue and groove, end matched.

 Color: [Wood Smoke.] [Timber Ridge.] [Natural.] [Lost Trail.] [Glacier.] [Black Forest.] [Big Sky.] [Back Country.] [To be selected from manufacturer’s full color range.]

 Surface texture: [Smooth.] [Wire brushed.]

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Vertical grain Hemlock

 Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

 Profile: Tongue and groove, end matched.

 Color: Natural.

 Surface texture: [Smooth.] [Wire brushed.]

 [Interior] [Exterior] Trim:

 Source: Evotrim

 Description: Engineered S4S, finger jointed and edge glued.

 Preservative treatment: TruCore.

 Species: Spruce/Pine/Fir.

 Thickness: Nominally [1 inch.] [1-1/4 inches.]

 Surface texture: [S1S2E.] [S4S.]

 Finish: Factory-applied primer with mildewcide.

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Source: True

 Description: Engineered S4S knot-free wood.

 Species: Cedar.

 Size: [\_\_ x \_\_] inches.

 Surface texture: Resawn one side; smooth sawn opposite side.

 Finish: Factory-applied two coat primer system

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Source: Premium Primed.

 Description: Solid sawn, finger jointed and edge glued, kiln dried.

 Species: Spruce/Pine/Fir.

 Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

 Surface texture: [S1S2E.] [S4S.]

 Preservative treatment: XTP Exterior Topical Preservative.

 Finish: Factory-applied primer with mildewcide.

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Source: Primed SPF

 Description: Solid sawn, kiln dried.

 Species: Spruce/Pine/Fir.

 Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

 Surface texture: [S1S2E.] [S4S.]

 Preservative treatment: XTP Exterior Topical Preservative.

 Finish: Factory-applied primer with mildewcide.

 ACCESSORIES

 Fasteners: [Hot dip galvanized steel.] [Aluminum.] [Type [304] [316] stainless steel.] [Fluoropolymer coated steel.] [\_\_\_\_].

 FABRICATION

 Quality: AWI Architectural Woodwork Standards, [Premium] [Custom] Grade.

 EXECUTION

 INSTALLATION

 Install trim in accordance with manufacturer’s instructions and AWI Architectural Woodwork Standards.

 [Butt] [Miter] ends, corners, and intersections.

END OF SECTION