SECTION 06 46 00 - WOOD TRIM

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes for trim.

Samples: [Selection samples.] [Verification samples.]

ADMINISTRATIVE REQUIREMENTS

Pre-Installation Conference:

Attendance: [Design Professional,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder,] installer, and related trades.

Review: Critical dimensions, delivery and storage, staging and sequencing, and protection of completed work.

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

Mockups: [[8] [\_\_] feet long.] [\_\_\_\_.] Approved mockups [may] [may not] remain as part of the Work.

WARRANTIES

Manufacturer’s 15 year warranty against peeling, checking, and chalking.

\*\*\*\* OR \*\*\*\*

Manufacturer’s 40 year warranty against rot, decay, and damage by insects or termites.

PRODUCTS

MANUFACTURERS

Wood Trim: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

[Interior] [Exterior] Trim:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Pine.

Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

Profile: Tongue and groove, end matched.

Color: [Wood Smoke.] [Timber Ridge.] [Natural.] [Lost Trail.] [Glacier.] [Black Forest.] [Big Sky.] [Back Country.] [To be selected from manufacturer’s full color range.]

Surface texture: [Smooth.] [Wire brushed.]

\*\*\*\* OR \*\*\*\*

[Interior] [Exterior] Trim:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Vertical grain Hemlock

Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

Profile: Tongue and groove, end matched.

Color: Natural.

Surface texture: [Smooth.] [Wire brushed.]

[Interior] [Exterior] Trim:

Source: Evotrim

Description: Engineered S4S, finger jointed and edge glued.

Preservative treatment: TruCore.

Species: Spruce/Pine/Fir.

Thickness: Nominally [1 inch.] [1-1/4 inches.]

Surface texture: [S1S2E.] [S4S.]

Finish: Factory-applied primer with mildewcide.

\*\*\*\* OR \*\*\*\*

[Interior] [Exterior] Trim:

Source: True

Description: Engineered S4S knot-free wood.

Species: Cedar.

Size: [\_\_ x \_\_] inches.

Surface texture: Resawn one side; smooth sawn opposite side.

Finish: Factory-applied two coat primer system

\*\*\*\* OR \*\*\*\*

[Interior] [Exterior] Trim:

Source: Premium Primed.

Description: Solid sawn, finger jointed and edge glued, kiln dried.

Species: Spruce/Pine/Fir.

Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

Surface texture: [S1S2E.] [S4S.]

Preservative treatment: XTP Exterior Topical Preservative.

Finish: Factory-applied primer with mildewcide.

\*\*\*\* OR \*\*\*\*

[Interior] [Exterior] Trim:

Source: Primed SPF

Description: Solid sawn, kiln dried.

Species: Spruce/Pine/Fir.

Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

Surface texture: [S1S2E.] [S4S.]

Preservative treatment: XTP Exterior Topical Preservative.

Finish: Factory-applied primer with mildewcide.

ACCESSORIES

Fasteners: [Hot dip galvanized steel.] [Aluminum.] [Type [304] [316] stainless steel.] [Fluoropolymer coated steel.] [\_\_\_\_].

FABRICATION

Quality: AWI Architectural Woodwork Standards, [Premium] [Custom] Grade.

EXECUTION

INSTALLATION

Install trim in accordance with manufacturer’s instructions and AWI Architectural Woodwork Standards.

[Butt] [Miter] ends, corners, and intersections.

END OF SECTION