SECTION 06 46 29 – WOOD SOFFITS

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes for cladding.

Samples: [Selection samples.] [Verification samples.]

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

WARRANTIES

PRODUCTS

MANUFACTURERS

Wood Wall and Ceiling Cladding: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Wood Soffits:

Source: Native Woods.

Description: Solid sawn.

Species: Engelman Spruce/Lodgepole Pine.

Size: Nominally 1 x 6 inches.

Profile: Tongue-and-groove, nickel gap, end matched.

Surface texture: Smooth.

Finish: [Natural.] [Alpine.] [Arctic Mist.] [Natural.] [Nightfall.] [Riverwash.] [Saddle.] [Whiskey Barrel.] [Gunmetal.] [Timberland.]

\*\*\*\* OR \*\*\*\*

Wood Soffits:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Ponderosa Pine.

Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

Profile: Tongue-and-groove, nickel gap, end matched.

Color: [Wood Smoke.] [Timber Ridge.] [Natural.] [Lost Trail.] [Glacier.] [Black Forest.] [Big Sky.] [Back Country.] [To be selected from manufacturer’s full color range.]

Surface texture: [Smooth.] [Wire brushed.]

\*\*\*\* OR \*\*\*\*

Wood Soffits:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Vertical grain Hemlock

Size: Nominally [1 x 4] [1 x 6] inches.

Profile: Tongue-and-groove, nickel gap, end matched.

Color: Natural.

Surface texture: [Smooth.] [Wire brushed.]

ACCESSORIES

Fasteners: Type [304] [316] stainless steel.

EXECUTION

INSTALLATION

Install soffits in accordance with manufacturer's instructions.

END OF SECTION