SECTION 06 46 29 – WOOD SOFFITS

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes for cladding.

 Samples: [Selection samples.] [Verification samples.]

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

 WARRANTIES

 PRODUCTS

 MANUFACTURERS

 Wood Wall and Ceiling Cladding: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

  Wood Soffits:

 Source: Native Woods.

 Description: Solid sawn.

 Species: Engelman Spruce/Lodgepole Pine.

 Size: Nominally 1 x 6 inches.

 Profile: Tongue-and-groove, nickel gap, end matched.

 Surface texture: Smooth.

 Finish: [Natural.] [Alpine.] [Arctic Mist.] [Natural.] [Nightfall.] [Riverwash.] [Saddle.] [Whiskey Barrel.] [Gunmetal.] [Timberland.]

\*\*\*\* OR \*\*\*\*

 Wood Soffits:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Ponderosa Pine.

 Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

 Profile: Tongue-and-groove, nickel gap, end matched.

 Color: [Wood Smoke.] [Timber Ridge.] [Natural.] [Lost Trail.] [Glacier.] [Black Forest.] [Big Sky.] [Back Country.] [To be selected from manufacturer’s full color range.]

 Surface texture: [Smooth.] [Wire brushed.]

\*\*\*\* OR \*\*\*\*

 Wood Soffits:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Vertical grain Hemlock

 Size: Nominally [1 x 4] [1 x 6] inches.

 Profile: Tongue-and-groove, nickel gap, end matched.

 Color: Natural.

 Surface texture: [Smooth.] [Wire brushed.]

 ACCESSORIES

 Fasteners: Type [304] [316] stainless steel.

 EXECUTION

 INSTALLATION

 Install soffits in accordance with manufacturer's instructions.

END OF SECTION