SECTION 07 46 23 - WOOD SIDING

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes for siding.

 Samples: [Selection samples.] [Verification samples.]

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

 WARRANTIES

 Manufacturer’s 20 year warranty against rot and decay.

 PRODUCTS

 MANUFACTURERS

 Wood Siding: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Wood Siding:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Ponderosa Pine.

 Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

 Profile: [Tongue and groove, nickel,gap reveal,] [Square edge,] end matched.

 Color: [Wood Smoke.] [Timber Ridge.] [Natural.] [Lost Trail.] [Glacier.] [Black Forest.] [Big Sky.] [Back Country.] [To be selected from manufacturer’s full color range.]

 Surface texture: [Smooth.] [Wire brushed.]

\*\*\*\* OR \*\*\*\*

 Wood Siding:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Vertical grain Hemlock

 Size: Nominally [1 x 4] [1 x 6] inches.

 Profile: [Tongue and groove, nickel gap reveal,] [Square edge,] end matched.

 Color: Natural.

 Surface texture: [Smooth.] [Wire brushed.]

 ACCESSORIES

 Fasteners: Type [304] [316] stainless steel.

 EXECUTION

 INSTALLATION

 Install siding in accordance with manufacturer's instructions.

 Install siding [horizontally.] [vertically.]

 [Miter end joints at 45 degrees.] [Butt end joints.]

 Install metal flashings at internal and external corners, sills, and heads of wall openings.

END OF SECTION