SECTION 09 78 31 – WOOD WALL AND CEILING CLADDING

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes for cladding.

Samples: [Selection samples.] [Verification samples.]

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

WARRANTIES

Manufacturer’s 20 year warranty against rot and decay.

PRODUCTS

MANUFACTURERS

Wood Wall and Ceiling Cladding: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Wood Wall and Ceiling Cladding:

Source: Native Woods.

Description: Solid sawn.

Species: Engelman Spruce/Lodgepole Pine.

Size: Nominally 1 x 6 inches.

Profile: Tongue-and-groove, nickel gap reveal, end matched.

Surface texture: Smooth.

Finish: [Natural.] [Alpine.] [Arctic Mist.] [Natural.] [Nightfall.] [Riverwash.] [Saddle.] [Whiskey Barrel.] [Gunmetal.] [Timberland.]

\*\*\*\* OR \*\*\*\*

Wood Wall and Ceiling Cladding:

Source: Timeless.

Description: Finger jointed, edge glued.

Species: Radiata Pine.

Size: Nominally 1 x 6 inches.

Profile: Tongue and groove, end matched.

Surface texture: Smooth.

Finish: [Natural.] [Midnight Black.] [Granite Gray.] [Farmhouse White.] [Cavalry Blue.]]

\*\*\*\* OR \*\*\*\*

Wood Wall and Ceiling Cladding:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Ponderosa Pine.

Size: Nominally [1 x 6] [1 x 8] inches.

Profile: Tongue and groove, nickel gap reveal, end matched.

Color: Natural.

Surface texture: [Smooth.] [Wire brushed.]

Finish: [Natural.] [Factory applied, [\_\_.]]

\*\*\*\* OR \*\*\*\*

Wood Wall and Ceiling Cladding:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Vertical grain Hemlock.

Size: Nominally 1 x 6 inches.

Profile: Tongue and groove, nickel gap reveal, end matched.

Finish: Natural.

Surface texture: [Smooth.] [Wire brushed.]

ACCESSORIES

Fasteners: [Steel.] [Hot dip galvanized steel.] [Aluminum.] [Type [304] [316] stainless steel.] [Fluoropolymer coated steel.] [\_\_\_\_].

EXECUTION

INSTALLATION

Install cladding in accordance with manufacturer's instructions.

Install cladding [horizontally.] [vertically.]

[Miter end joints at 45 degrees.] [Butt end joints.]

END OF SECTION