SECTION 08 78 13 – BARN DOOR HARDWARE

 GENERAL

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes.

 QUALITY ASSURANCE

 Installer Qualifications: Minimum [2] [\_\_] years’ experience in installation of door hardware.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by C.R. Laurence. [www.crlaurence.com](http://www.crlaurence.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 COMPONENTS

 Barn Door Hardware:

 Source: Latitude 34 Barn Door Collection – Hemisphere Sliding Door.

 Capacity: 200 pounds.

 Tested to 1 million cycles.

 6005A-T61 and 6061-T6 alloy aluminum construction.

 Concealed fasteners and trolley.

 Adjustable track height, door stops, and sliding resistance.

\*\*\* OR \*\*\*

 Barn Door Hardware:

 Source: Latitude 34 Barn Door Collection – Meridian Sliding Door.

 Capacity: 400 pounds.

 Tested to 1 million cycles.

 6005A-T61 and 6061-T6 alloy aluminum construction.

 Concealed track fasteners and ball bearings.

 Adjustable door height, track height, and door stops.

\*\*\* OR \*\*\*

 Barn Door Hardware:

 Source: Latitude 34 Barn Door Collection – Solstice Sliding Door.

 Capacity: 550 pounds.

 Tested to 1 million cycles.

 6005A-T61 and 6061-T6 alloy aluminum construction.

 Concealed track fasteners.

 Adjustable glass pane height, track height, and door stops.

 FINISHES

 Barn Door Hardware: [Black stainless.] [Brushed stainless.]

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer's instructions and approved Shop Drawings.

END OF SECTION