SECTION 08 78 13 – BARN DOOR HARDWARE

GENERAL

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes.

QUALITY ASSURANCE

Installer Qualifications: Minimum [2] [\_\_] years’ experience in installation of door hardware.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by C.R. Laurence. [www.crlaurence.com](http://www.crlaurence.com)

Substitutions: [Refer to Division 01.] [Not permitted.]

COMPONENTS

Barn Door Hardware:

Source: Latitude 34 Barn Door Collection – Hemisphere Sliding Door.

Capacity: 200 pounds.

Tested to 1 million cycles.

6005A-T61 and 6061-T6 alloy aluminum construction.

Concealed fasteners and trolley.

Adjustable track height, door stops, and sliding resistance.

\*\*\* OR \*\*\*

Barn Door Hardware:

Source: Latitude 34 Barn Door Collection – Meridian Sliding Door.

Capacity: 400 pounds.

Tested to 1 million cycles.

6005A-T61 and 6061-T6 alloy aluminum construction.

Concealed track fasteners and ball bearings.

Adjustable door height, track height, and door stops.

\*\*\* OR \*\*\*

Barn Door Hardware:

Source: Latitude 34 Barn Door Collection – Solstice Sliding Door.

Capacity: 550 pounds.

Tested to 1 million cycles.

6005A-T61 and 6061-T6 alloy aluminum construction.

Concealed track fasteners.

Adjustable glass pane height, track height, and door stops.

FINISHES

Barn Door Hardware: [Black stainless.] [Brushed stainless.]

EXECUTION

INSTALLATION

Install in accordance with manufacturer's instructions and approved Shop Drawings.

END OF SECTION