Scepter Developed by ZeroDocs.com

SECTION 01 56 26 – TEMPORARY FENCING

GENERAL

ADMINISTRATIVE REQUIREMENTS

Pre-Installation Conference:

Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] and fence installer.

Review: Project conditions, proposed fencing locations, and installation schedule.

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes.

Samples: Verification samples.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by Scepter, [www.scepterposts.com](http://www.scepterposts.com).

Substitutions: [Refer to Division 01.] [Not permitted.]

COMPONENTS

Fence Posts:

Product: Scepter Post, Multi-Fence Heavy Duty.

Length: 60 inches.

\*\*\*\* OR \*\*\*\*

Fence Posts:

Product: Scepter Post, Standard Heavy Duty.

Length: 60 inches.

\*\*\*\* OR \*\*\*\*

Fence Posts:

Product: Scepter Post, Multi-Fence Lite.

Length: 60 inches.

\*\*\*\* OR \*\*\*\*

Fence Posts:

Product: Scepter Post, Standard Lite.

Length: 60 inches.

\*\*\*\* OR \*\*\*\*

Fence Posts:

Product: Scepter Post, Silt Pole HD.

Length: 39.4 inches.

Fence Mesh:

Product: Barrier Fence.

Height: 48 inches.

Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

Fence Mesh:

Product: Barricade Fence.

Height: 48 inches.

Opening size: 1.5 x 2.5 inches.

Thickness: 0.0125 inch.

\*\*\*\* OR \*\*\*\*

Fence Mesh:

Product: Snow Control Fence.

Height: 48 inches.

\*\*\*\* OR \*\*\*\*

Fence Mesh:

Product: Snow Fence.

Height: 48 inches.

Opening size: 1.25 x 2 inches.

\*\*\*\* OR \*\*\*\*

Fence Mesh:

Product: Yard Fence.

Height:48 inches.

Opening size: 1.5 x 1.5 inches.

\*\*\*\* OR \*\*\*\*

Fence Fabric:

Product: Silt Fence.

Height: 36 inches.

Sieve size: No. 30 (0.023 inch).

Caution Tape:

Product: Caution Tape.

Height: \_\_\_\_ inches.

Color: [Red.] [Yellow.]

Lettering: [CAUTION.] [DANGER.] [DO NOT ENTER.]

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions.

Maximum fence post spacing: [\_\_] feet on center.

END OF SECTION