PROSOCO, Inc. Distributed by ZeroDocs.com

SECTION 09 96 23 – GRAFFITI REMOVAL

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes.

 Closeout Submittals:

 Maintenance Data.

 QUALITY ASSURANCE

 Applicator Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

 Mockup: Minimum [\_\_x \_\_] feet.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by PROSOCO, Inc. [www.PROSOCO.com](http://www.prosoco.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Graffiti Remover:

 Product: Sure Klean Graffiti Remover.

 Description: VOC compliant graffiti remover.

\*\*\*\* OR \*\*\*\*

 Graffiti Remover:

 Product: Enviro Klean Safstrip.

 Description: VOC compliant cleaner and paint stripper.

\*\*\*\* OR \*\*\*\*

 Graffiti Remover:

 Product: Enviro Klean Safstrip 8.

 Description: Neutral pH graffiti remover.

 EXECUTION

 APPLICATION

 Apply in accordance with manufacturer's instructions.

END OF SECTION