PROSOCO, Inc. Distributed by ZeroDocs.com

SECTION 09 96 23 – GRAFFITI REMOVAL

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes.

Closeout Submittals:

Maintenance Data.

QUALITY ASSURANCE

Applicator Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

Mockup: Minimum [\_\_x \_\_] feet.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by PROSOCO, Inc. [www.PROSOCO.com](http://www.prosoco.com)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Graffiti Remover:

Product: Sure Klean Graffiti Remover.

Description: VOC compliant graffiti remover.

\*\*\*\* OR \*\*\*\*

Graffiti Remover:

Product: Enviro Klean Safstrip.

Description: VOC compliant cleaner and paint stripper.

\*\*\*\* OR \*\*\*\*

Graffiti Remover:

Product: Enviro Klean Safstrip 8.

Description: Neutral pH graffiti remover.

EXECUTION

APPLICATION

Apply in accordance with manufacturer's instructions.

END OF SECTION