MB Sentinel Developed by ZeroDocs.com

SECTION 10 85 00 – PACKAGE TRANSFERS

 GENERAL

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes.

 Samples: [Selection samples.] [Verification samples.]

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by MB Sentinel, [www.mbsentinel.com](http://www.mbsentinel.com).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MANUFACTURED UNITS

 Package Transfers:

 Model: Box Gobbler [1428.] [2828.]

 Size: [14 inches wide x 28 inches high.] [28 inches wide x 28 inches high.]

 Construction:

* + - * 1. Frame and door: 0.125 inch thick aluminum.
				2. Chute: 12 gage stainless steel.
				3. Conveyors: Stainless steel rod and PVC.
				4. Door handle: 16 gage stainless steel.
				5. Door: Bottom hinged with positive stop, self-closing, with 2 inch insulation.
				6. Access panel back plate: 0.60 inch thick aluminum, powder coated, non-insulated.
				7. Hinges: [Exposed, nylon.] [Concealed, stainless-steel hinge by SOSS.]

 Lock: [4 to 6 digit keypad controller and electronic rotary latch.] [No lock.]

 Finish: Manufacturer’s standard powder coat, [[custom] [\_\_\_\_] color.] [Color to be selected from manufacturer’s full color range.] [Unfinished.]

 ACCESSORIES

 Fasteners: Type best suited to application, [galvanized steel.] [corrosion resistant coated steel.] [Series 300 stainless steel.]

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions and approved Shop Drawings.

END OF SECTION